{"text_format":"3","workbook":"xls","n_sheets":6,"sheets":["RVO2","RVO3","RVO4","RVO 5","RVO6","Súhrn"],"not_rendered":{"external_links":1,"defined_names":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RVO2","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"flags":["formulas_cached_only"]}
["Popis","MJ","Množstvo","Cena jednotková","Materiál","Montáž","Ostatné","Cena celkom"]
[{"$nulls":3},"EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH"]
["DEMONTÁŽNE PRÁCE"]
["Demontáž svietidla","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Odvoz a likvidácia","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["MONTÁŽNE PRÁCE"]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED30-4S/730 DM12 - 19,8W","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Svietidlo LED","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre oceľové stožiare ","m",{"v":43.5,"d":"43.50"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre oceľové stožiare ","m",{"v":43.5,"d":"43.50"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL3","ks",{"v":87,"d":"87.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL3","ks",{"v":87,"d":"87.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Stožiarová svorkovnica  TB-1 stožiarová bez poistky 4 žily","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Poistka valcová 500V AC, 6A, 100kA, gG - poistka 6A D01 E14 do stožiarovej svorkovnice","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž svorkovnice stožiarovej, pripevnenie svorkovnice, úprava káblov, montáž do 15 ks vodičov do priemeru 16 mm, montáž poistky, zapojenie vývodu pre svietidlo, uzatvorenie svorkovnice min IP 43.","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Ukončenie vodičov . vč. zapojenia a vodičovej koncovky do 16 mm2","ks",{"v":319,"d":"319.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Náter a odhrdzavenie oceľového stožiara","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Farba RAL 9006 Alkyton","l",{"v":21,"d":"21.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["RVO",null,null,{"v":0,"d":"0.00"}]
["Úprava v rozvádzači - montáž","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Úprava v rozvádzači RVO - výmena prístrojov a inštalácie - materiál (zvodič prepätia B+C, astrohodiny, prepínač R-O-A, ističe)","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Analýza a optimalizácia MRK RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pripojovacie poplatky spojené s rekonštrukciou VO","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["OSTATNÉ"]
["Podružný materiál","%",{"v":1.5,"d":"1.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Podiel pridružených výkonov","%",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Inžiniering pre rekonštrukciu VO ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia osvetľovacej sústavy ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina","hod",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina pre náter stožiarov","hod.",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava plošina","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Celkom bez DPH",{"$nulls":3},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00"}]
["DPH (20%)",{"$nulls":6},{"v":0,"d":"0.00"}]
["Celkom s DPH",{"$nulls":6},{"v":0,"d":"0.00"}]

{"sheet":"RVO3","index":1,"n_rows":29,"n_cols":8,"rows_kept":29,"flags":["formulas_cached_only"]}
["Popis","MJ","Množstvo","Cena jednotková","Materiál","Montáž","Ostatné","Cena celkom"]
[{"$nulls":3},"EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH"]
["DEMONTÁŽNE PRÁCE"]
["Demontáž svietidla","ks",{"v":54,"d":"54.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Odvoz a likvidácia","ks",{"v":54,"d":"54.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["MONTÁŽNE PRÁCE"]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED30-4S/730 DM12 - 19,8W","ks",{"v":54,"d":"54.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Svietidlo LED","ks",{"v":54,"d":"54.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre oceľové stožiare ","m",{"v":81,"d":"81.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL3","ks",{"v":162,"d":"162.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL3","ks",{"v":162,"d":"162.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre oceľové stožiare ","m",{"v":81,"d":"81.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["RVO"]
["Úprava v rozvádzači - montáž","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Úprava v rozvádzači RVO - výmena prístrojov a inštalácie - materiál (zvodič prepätia B+C, astrohodiny, prepínač R-O-A, ističe)","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Analýza a optimalizácia MRK RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pripojovacie poplatky spojené s rekonštrukciou VO","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["OSTATNÉ"]
["Podružný materiál","%",{"v":1.5,"d":"1.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Podiel pridružených výkonov","%",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Inžiniering pre rekonštrukciu VO ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia osvetľovacej sústavy ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina","hod",{"v":54,"d":"54.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava plošina","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Celkom bez DPH",{"$nulls":3},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00"}]
["DPH (20%)",{"$nulls":6},{"v":0,"d":"0.00"}]
["Celkom s DPH",{"$nulls":6},{"v":0,"d":"0.00"}]

{"sheet":"RVO4","index":2,"n_rows":74,"n_cols":8,"rows_kept":74,"flags":["formulas_cached_only"]}
["Popis","MJ","Množstvo","Cena jednotková","Materiál","Montáž","Ostatné","Cena celkom"]
[{"$nulls":3},"EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH"]
["DEMONTÁŽNE PRÁCE"]
["Demontáž svietidla","ks",{"v":72,"d":"72.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Odvoz a likvidácia","ks",{"v":72,"d":"72.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["MONTÁŽNE PRÁCE"]
["Hliníkový výložník WR-4/1/1,0/5 anodizácia inox","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Výložník","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Reflektor LED Coreline Tempo BVP130 LED120-4S/740 A","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED30-4S/730 DM12 - 19,8W","ks",{"v":74,"d":"74.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Svietidlo LED","ks",{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Poistkové púzdro vrátane poistky 2A ","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž poistkového púzdra","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre výložník","m",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre výložník","m",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre oceľové stožiare ","m",{"v":120.5,"d":"120.50"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre oceľové stožiare ","m",{"v":120.5,"d":"120.50"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL3","ks",{"v":225,"d":"225.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL3","ks",{"v":225,"d":"225.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Výkop v chodníku do hĺbky 80 cm, odvoz výkopku na skládku, pokládka kábla, fólia, zásyp, uvedenie do pôvodného stavu","m",{"v":35,"d":"35.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Fólia BLESK  30cm  výstražná červená ","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Kábel silový s Cu jadrom CYKY-J 4x10","m",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - silový kábel Cu 750-1000 V (v mm2) CYKY 1 kV do 4x50","m",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rúrka KF 09040 BA dvojplášťová  červená KOPOFLEX 40 - chránička káblová ohybná, spevnená","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka chráničky priemeru do 50mm do výkopu","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Guľatina FeZn8 (1kg=2,5m, 1m=0,4kg), vrátane podružného materiálu","kg",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SP1 pripojovacia  pre spojenie kovových súčiastok, d=8-10mm","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SJ02 4xM8 k zemniacej tyči , d=25mm","ks",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Uzemnenie stožiara vrátane svoriek","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Tyč ZT 1,5m uzemňovacia plná","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - výkop jamy pre stožiar do výšky 8m","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Stožiarová svorkovnica  TB-1 stožiarová bez poistky 4 žily","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Stožiarová svorkovnica  TB-2 stožiarová bez poistiek 4 žily","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Poistka valcová 500V AC, 6A, 100kA, gG - poistka 6A D01 E14 do stožiarovej svorkovnice","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž svorkovnice stožiarovej, pripevnenie svorkovnice, úprava káblov, montáž do 15 ks vodičov do priemeru 16 mm, montáž poistky, zapojenie vývodu pre svietidlo, uzatvorenie svorkovnice min IP 43.","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Ukončenie vodičov . vč. zapojenia a vodičovej koncovky do 16 mm2","ks",{"v":22,"d":"22.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Stožiar prírubový hliníkový výšky 8 m typ SAL-80K v úprave anodizovaný hliník ","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["betónový základ B-71 vr.spojovacích prvkov B-70,B-71, B-80","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Základ pre stožiar prírubový verejného osvetlenia v ose trasy kábla do výšky 8m","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Montáž stožiara do výšky 8 m, doprava (z blizkej skladky) a montáž stožiara, osadenie do základu,zatiahnutie kábla, zhotovenie čapice","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Asfaltový náter pri uzemnení","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Opatrenie vývodov zo zeme ochranným náterom","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["RVO"]
["Úprava v rozvádzači - montáž","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Úprava v rozvádzači RVO - výmena prístrojov a inštalácie - materiál (zvodič prepätia B+C, astrohodiny, prepínač R-O-A, ističe)","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Analýza a optimalizácia MRK RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pripojovacie poplatky spojené s rekonštrukciou VO","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["MONTÁŽ SAMONOSNÉHO KÁBLA"]
["Samonosný kábel CYMYz 2x2,5","m",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Samonosný kábel do 25mm2","m",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Záves kotevný Z-CK","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Záves kotevný Z-CK","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Záves kotevný Z-CP","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Záves kotevný Z-CP","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rozvodka 6455-11 4.P/2 FUTURE IP67 (ACIDUR) krabicová-svetlosivá, 5 pól, tesn. rozsah 7-16mm","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž Acedur","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL5","ks",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL5","ks",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL3","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL3","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["OSTATNÉ"]
["Podružný materiál","%",{"v":1.5,"d":"1.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Podiel pridružených výkonov","%",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Odvoz sutiny na skládku","m3",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Inžiniering pre rekonštrukciu VO ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia osvetľovacej sústavy ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava stožiarov","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina","hod",{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava plošina","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Celkom bez DPH",{"$nulls":3},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00"}]
["DPH (20%)",{"$nulls":6},{"v":0,"d":"0.00"}]
["Celkom s DPH",{"$nulls":6},{"v":0,"d":"0.00"}]

{"sheet":"RVO 5","index":3,"n_rows":55,"n_cols":8,"rows_kept":55,"flags":["formulas_cached_only"]}
["Popis","MJ","Množstvo","Cena jednotková","Materiál","Montáž","Ostatné","Cena celkom"]
[{"$nulls":3},"EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH"]
["DEMONTÁŽNE PRÁCE"]
["Demontáž svietidla","ks",{"v":79,"d":"79.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž výložníka pod vedením NN","ks",{"v":79,"d":"79.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Odvoz a likvidácia","ks",{"v":159,"d":"159.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž RVO ","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["MONTÁŽNE PRÁCE"]
["Výložník na betonový stožiar V05A (VBS 1/50cm A)","ks",{"v":78,"d":"78.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Výložník na betonový stožiar V05B (VBS 1/50cm B)","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Výložník na betonový stožiar V05C (VBS 1/50cm C)","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Výložník na betonový stožiar V10B (VBS 1/100cm B)","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Výložník","ks",{"v":91,"d":"91.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED30-4S/730 DM12 - 19,8W","ks",{"v":83,"d":"83.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED27-4S/730 DM12 - 17,8 W","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Svietidlo LED","ks",{"v":91,"d":"91.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka prepichovacia izolovaná malá 16-95/1,5-10","ks",{"v":182,"d":"182.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Prepichovacia/univerzálna svorka","ks",{"v":182,"d":"182.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Poistkové púzdro vrátane poistky 2A ","ks",{"v":91,"d":"91.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž poistkového púzdra","ks",{"v":91,"d":"91.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre výložník","m",{"v":455,"d":"455.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre výložník","m",{"v":455,"d":"455.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["RVO",null,null,{"v":0,"d":"0.00"}]
["Rozvádzač RVO - pilierový - hl.istič, istenie vývodov, prívod a vývody odspodu, astrohodiny, zvodič prapätia B+C, svetlo, zásuvka,  prepínač R-0-A","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Rozvádzač RVO, do 3x63A/400V pilierový","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Uzemnenie RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Tyč ZT 1,5m uzemňovacia plná","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SJ02 4xM8 k zemniacej tyči , d=25mm","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Guľatina FeZn10 (1kg=1,612m, 1m=0,62kg), vrátane podružného materiálu","kg",2.17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka uzemňovacieho vedenia,  FeZn30/4 alebo FeZn ø=10 mm2 alebo v FeZn ø=8 mm2 zemi včít. svoriek,prepojenia, izolácie spojov s FeZn ø=10 mm","kg",2.17,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Ukončenie vodičov . vč. zapojenia a vodičovej koncovky do 25 mm2","ks",{"v":24,"d":"24.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rúrka KF 09050 BA dvojplášťová  červená KOPOFLEX 50 - chránička káblová ohybná, spevnená","m",{"v":11,"d":"11.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka chráničky priemeru do 63mm do výkopu","m",{"v":11,"d":"11.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Výkop v chodníku do hĺbky 70 cm, odvoz výkopku na skládku, pokládka kábla, fólia, piesok, zásyp, uvedenie do pôvodného stavu","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Fólia BLESK  30cm  výstražná červená  ","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Silový kábel hliníkový 750-1000 V (v mm2) voľne uložený AYKY 1 kV do 4x25","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel 1- AYKY-J 4x25 - silový s hliníkovým jadrom","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka prepichovacia 16-70/4-35 MM2 (Plamen P43-20-31 (P43-21-31))","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Prepichovacia svorka na káblové vedenia ","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Analýza a optimalizácia MRK RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Sada SZT-SKS 3/4 zmršťovacia s trhacími spojkami 4x16-25mm do 1kV","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - káblová spojka pre zabudované rozvádzače","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pripojovacie poplatky spojené s rekonštrukciou VO","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["OSTATNÉ"]
["Podružný materiál","%",{"v":1.5,"d":"1.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Podiel pridružených výkonov","%",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Inžiniering pre rekonštrukciu VO ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia osvetľovacej sústavy ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina","hod",{"v":91,"d":"91.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava plošina","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Celkom bez DPH",{"$nulls":3},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00"}]
["DPH (20%)",{"$nulls":6},{"v":0,"d":"0.00"}]
["Celkom s DPH",{"$nulls":6},{"v":0,"d":"0.00"}]

{"sheet":"RVO6","index":4,"n_rows":148,"n_cols":8,"rows_kept":148,"flags":["formulas_cached_only"]}
["Popis","MJ","Množstvo","Cena jednotková","Materiál","Montáž","Ostatné","Cena celkom"]
[{"$nulls":3},"EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH"]
["DEMONTÁŽNE PRÁCE"]
["Demontáž svietidla","ks",{"v":53,"d":"53.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž výložníka pod vedením NN","ks",{"v":33,"d":"33.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Odvoz a likvidácia","ks",{"v":129,"d":"129.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž RVO ","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž oceľového stožiara / oceľovo-betónového stožiara do 5m ","ks",{"v":21,"d":"21.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž základu stožiara -spevneny povrch","ks",{"v":21,"d":"21.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["MONTÁŽNE PRÁCE"]
["Výložník na betonový stožiar V05A (VBS 1/50cm A)","ks",{"v":37,"d":"37.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Výložník na betonový stožiar V05B (VBS 1/50cm B)","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Výložník na betonový stožiar V05C (VBS 1/50cm C)","ks",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Výložník na betonový stožiar V10A (VBS 1/100cm A)","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Hliníkový výložník WR-4/1/1,0/5 anodizácia inox","ks",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Hliníkový výložník WRP-1/1,5/1,2/5 anodizácia inox","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Výložník","ks",{"v":66,"d":"66.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED60-4S/730 DM12 - 38,5W","ks",{"v":24,"d":"24.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED30-4S/730 DM12 - 19,8W","ks",{"v":11,"d":"11.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED27-4S/730 DM12 - 17,8 W","ks",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet gen2 mini BGP282 T25 1 xLED39-4S/730 DM12 - 25,5W","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Svietidlo LED","ks",{"v":66,"d":"66.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka prepichovacia izolovaná malá 16-95/1,5-10","ks",{"v":104,"d":"104.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Prepichovacia/univerzálna svorka","ks",{"v":104,"d":"104.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Poistkové púzdro vrátane poistky 2A ","ks",{"v":94,"d":"94.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž poistkového púzdra","ks",{"v":94,"d":"94.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre výložník","m",{"v":380,"d":"380.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre výložník","m",{"v":380,"d":"380.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5 pre oceľové stožiare ","m",{"v":219,"d":"219.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5 pre oceľové stožiare ","m",{"v":219,"d":"219.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Výkop v zeleni do hĺbky 80 cm, zatrávnenie, odvoz výkopku na skládku, pokládka kábla, fólia,zásyp, uvedenie do pôvodného stavu","m",{"v":296,"d":"296.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Výkop v chodníku do hĺbky 80 cm, odvoz výkopku na skládku, pokládka kábla, fólia, zásyp, uvedenie do pôvodného stavu","m",{"v":415,"d":"415.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Fólia BLESK  30cm  výstražná červená ","m",{"v":750,"d":"750.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Kábel silový s Cu jadrom CYKY-J 4x10","m",{"v":1026,"d":"1026.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - silový kábel Cu 750-1000 V (v mm2) CYKY 1 kV do 4x50","m",{"v":1026,"d":"1026.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rúrka KF 09040 BA dvojplášťová  červená KOPOFLEX 40 - chránička káblová ohybná, spevnená","m",{"v":850,"d":"850.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka chráničky priemeru do 50mm do výkopu","m",{"v":850,"d":"850.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rúrka 6036 ZNM ocelová závitová pozinkovaná 3m - materiál","ks",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Rúrka 6036 ZNM ocelová závitová pozinkovaná 3m - montáž","ks",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Koleno 6136 ZNM D pre ocelové rúrky - materiál","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Koleno 6136 ZNM D pre ocelové rúrky - montáž","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["SPOJKY PRE OCELOVE ZAVITOVE RURKY -1/50 N1-M0-P0 - materiál","ks",{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["SPOJKY PRE OCELOVE ZAVITOVE RURKY -1/50 N1-M0-P0 - montáž","ks",{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pokládka uzemňovacieho vedenia,  FeZn30/4 alebo FeZn ø=10 mm2 alebo v FeZn ø=8 mm2 zemi včít. svoriek,prepojenia, izolácie spojov s FeZn ø=10 mm","m",{"v":727.5,"d":"727.50"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Guľatina FeZn8 (1kg=2,5m, 1m=0,4kg), vrátane podružného materiálu","kg",{"v":27,"d":"27.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Guľatina FeZn10 (1kg=1,612m, 1m=0,62kg), vrátane podružného materiálu","kg",{"v":409.4292803970223,"d":"409"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SP1 pripojovacia  pre spojenie kovových súčiastok, d=8-10mm","ks",{"v":29,"d":"29.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SS spojovacia bez príložky s 2 skrutkami d=8-10mm","ks",{"v":91.37717121588089,"d":"91"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SJ02 4xM8 k zemniacej tyči , d=25mm","ks",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Uzemnenie stožiara vrátane svoriek","ks",{"v":24,"d":"24.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Tyč ZT 1,5m uzemňovacia plná","ks",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - výkop jamy pre stožiar do výšky 8m","ks",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Montáž - výkop jamy pre stožiar do výšky 12m","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Stožiarová svorkovnica  TB-1 stožiarová bez poistky 4 žily","ks",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Poistka valcová 500V AC, 6A, 100kA, gG - poistka 6A D01 E14 do stožiarovej svorkovnice","ks",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž svorkovnice stožiarovej, pripevnenie svorkovnice, úprava káblov, montáž do 15 ks vodičov do priemeru 16 mm, montáž poistky, zapojenie vývodu pre svietidlo, uzatvorenie svorkovnice min IP 43.","ks",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Ukončenie vodičov . vč. zapojenia a vodičovej koncovky do 16 mm2","ks",{"v":275,"d":"275.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Stožiar prírubový hliníkový výšky 8 m typ SAL-80K v úprave anodizovaný hliník ","ks",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["betónový základ B-71 vr.spojovacích prvkov B-70,B-71, B-80","ks",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Stožiar prírubový hliníkový výšky 9 m typ SAL-90M v úprave anodizácia inox","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["betónový základ B-71 vr.spojovacích prvkov","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Základ pre stožiar prírubový verejného osvetlenia v ose trasy kábla do výšky 8m","ks",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Základ pre stožiar prírubový verejného osvetlenia v ose trasy kábla do výšky 12 m","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Montáž stožiara do výšky 8 m, doprava (z blizkej skladky) a montáž stožiara, osadenie do základu,zatiahnutie kábla, zhotovenie čapice","ks",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Montáž stožiara do výšky 12 m, doprava (z blizkej skladky), osadenie do základu,zatiahnutie kábla","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Asfaltový náter pri uzemnení","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Opatrenie vývodov zo zeme ochranným náterom","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["RVO"]
["Rozvádzač RVO - pilierový - hl.istič, istenie vývodov, prívod a vývody odspodu, astrohodiny, zvodič prapätia B+C, svetlo, zásuvka,  prepínač R-0-A","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Rozvádzač RVO, do 3x63A/400V pilierový","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Uzemnenie RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Tyč ZT 1,5m uzemňovacia plná","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SJ02 4xM8 k zemniacej tyči , d=25mm","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Guľatina FeZn10 (1kg=1,612m, 1m=0,62kg), vrátane podružného materiálu","kg",2.17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka uzemňovacieho vedenia,  FeZn30/4 alebo FeZn ø=10 mm2 alebo v FeZn ø=8 mm2 zemi včít. svoriek,prepojenia, izolácie spojov s FeZn ø=10 mm","kg",2.17,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Ukončenie vodičov . vč. zapojenia a vodičovej koncovky do 25 mm2","ks",{"v":64,"d":"64.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rúrka KF 09050 BA dvojplášťová  červená KOPOFLEX 50 - chránička káblová ohybná, spevnená","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka chráničky priemeru do 63mm do výkopu","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Výkop v chodníku do hĺbky 70 cm, odvoz výkopku na skládku, pokládka kábla, fólia, piesok, zásyp, uvedenie do pôvodného stavu","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Fólia BLESK  30cm  výstražná červená  ","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Silový kábel hliníkový 750-1000 V (v mm2) voľne uložený AYKY 1 kV do 4x25","m",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel 1- AYKY-J 4x25 - silový s hliníkovým jadrom","m",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka prepichovacia 16-70/4-35 MM2 (Plamen P43-20-31 (P43-21-31))","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Prepichovacia svorka na káblové vedenia ","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Analýza a optimalizácia MRK RVO","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Sada SZT-SKS 3/4 zmršťovacia s trhacími spojkami 4x16-25mm do 1kV","ks",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - káblová spojka pre zabudované rozvádzače","ks",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pripojovacie poplatky spojené s rekonštrukciou VO","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["ROZHLAS A ROZHLASOVÉ VEDENIE"]
["Demontáž reproduktorov rozhlasu ","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž vedenia rozhlasu ","m",{"v":620,"d":"620.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Demontáž konzól rozhlasu","ks",{"v":22,"d":"22.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Konzoly rozhlasu","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž konzôl rozhlasu","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Montáž reproduktorov rozhlasu ","ks",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x2,5 (pre rozhlas - Hlavná ulica)","m",{"v":792,"d":"792.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x2,5 (pre rozhlas - Hlavná ulica)","m",{"v":792,"d":"792.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Trubka FXP 25 - chránička káblová ohybná, spevnená","m",{"v":670,"d":"670.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Pokládka chráničky priemeru do 25mm do výkopu","m",{"v":670,"d":"670.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Napojenie nového káblového rozvodu pre rozhlas","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["OSVETLENIE PRIECHODOV PRE CHODCOV"]
["Vypracovanie projektovej dokumentácie  osvetlenia priechodov pre stavebné povolenie","kpl",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Výložník na oceľový stožiar UD Z 2 3000","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Výložník","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svietidlo LED UniStreet BGP282 LED109_757_prechod_67W","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Svietidlo LED","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Poistkové púzdro vrátane poistky 2A ","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž poistkového púzdra","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Kábel silový medený CYKY-J  3x1,5","m",{"v":36,"d":"36.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Kábel silový medený CYKY-J 3x1,5","m",{"v":36,"d":"36.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Pokládka uzemňovacieho vedenia,  FeZn30/4 alebo FeZn ø=8 mm2 v zemi včít. svoriek,prepojenia, izolácie spojov s FeZn ø=8 mm","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Guľatina FeZn8 (1kg=2,5m, 1m=0,4kg), vrátane podružného materiálu","kg",{"v":2.5,"d":"2.50"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SP1 pripojovacia  pre spojenie kovových súčiastok, d=8-10mm","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Svorka SJ02 4xM8 k zemniacej tyči , d=25mm","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Asfaltový náter pri uzemnení","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Opatrenie vývodov zo zeme ochranným náterom","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Uzemnenie stožiara vrátane svoriek","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Tyč ZT 1,5m uzemňovacia plná","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - výkop jamy pre stožiar","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Stožiar STP 6 - CZ 159/133/114 - bezprírubový oceľový zinkovaný výšky 6m","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž stožiara do výšky 6 m, osadenie do základu,zatiahnutie kábla, zhotovenie čapice",null,{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["MONTÁŽ SAMONOSNÉHO KÁBLA PRE PRIECHODY"]
["Samonosný kábel CYMYz 2x2,5","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Samonosný kábel do 25mm2","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Záves kotevný Z-CK ","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž - Záves kotevný Z-CK","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Rozvodka 6455-11 4.P/2 FUTURE IP67 (ACIDUR) krabicová-svetlosivá, 5 pól, tesn. rozsah 7-16mm","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž Acedur","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL5","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL5","ks",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["Svorka WAGO FKL3","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"}]
["Montáž WAGO FKL3","ks",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
["OSTATNÉ"]
["Podružný materiál","%",{"v":1.5,"d":"1.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Podiel pridružených výkonov","%",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Odvoz sutiny na skládku","m3",98.75,{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Asfaltovanie min 4 cm hrubého asfaltu, 3 cm jemného asfaltu s vyrovnaním terénu","m2",{"v":224.5,"d":"224.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Inžiniering pre rekonštrukciu VO ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia","ks",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Revízia osvetľovacej sústavy ","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava stožiarov","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina","hod",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Montážna plošina pre rozhlas","hod",{"v":5.5,"d":"5.50"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Doprava plošina","kpl",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},null,null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Celkom bez DPH",{"$nulls":3},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00"}]
["DPH (20%)",{"$nulls":6},{"v":0,"d":"0.00"}]
["Celkom s DPH",{"$nulls":6},{"v":0,"d":"0.00"}]

{"sheet":"Súhrn","index":5,"n_rows":10,"n_cols":6,"rows_kept":10,"flags":["formulas_cached_only"]}
["Popis","MJ","Materiál","Montáž","Ostatné","Cena celkom"]
[null,null,"EUR bez DPH","EUR bez DPH","EUR bez DPH","EUR bez DPH"]
["RVO2",null,0,0,0,0]
["RVO3",null,0,0,0,0]
["RVO4",null,0,0,0,0]
["RVO5",null,0,0,0,0]
["RVO6",null,{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},{"v":0,"d":"0.00 €"},0]
["Celkom bez DPH",null,{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},{"v":0,"d":"0.000"}]
["DPH (20%)",{"$nulls":4},{"v":0,"d":"0.00"}]
["Celkom s DPH",{"$nulls":4},{"v":0,"d":"0.00"}]